# Rack mounting Symphony I/O

Rack ears are included in the Accessories box for mounting Symphony I/O in a standard 19” equipment rack.

> 1. Orient one rack ear to line up the ear's three holes with three holes found on the side of the chassis immediately behind the front panel extrusion.

> 2. Insert 3 screws (included) and finger tighten.

> 3. Connect the second rack ear to the other side of the chassis.

> 4. On each side, line up the top and bottom of the rack ear with the top and bottom of the front panel extrusion and tighten the screws with a Phillips screwdriver. Don't overtighten the screws.

> 5. Remove the screw-on feet by turning them counter-clockwise by hand or with a Philips screwdriver.

##