# Mixer Tab Window

Use the Mixer Tab Window to adjust the Mix of input and output signals as well as configure Low Latency Mixing. Learn more about Low Latency Mixing.

> > 1. Device Icon & ID Button - see the description above.
> > 2. Pan - This rotary knob pans the input signal between he left and right sides of the Maestro mixer's stereo output.
> > 3. Input Level fader - This slider sets the level of the input signal in the Maestro mixer's stereo output.
> > 4. Meter - This bargraph style meter displays the pre-fader input level.
> > 5. Level Value Window - The level value, between -48 and 0 dBFS.
> > 6. Solo - This button mutes all other channels whose Solo buttons are not engaged.
> > 7. Mute - This button mutes the input channel.
> > 8. Software Return Fader - This stereo input channel provides level control, metering, and mute/solo functions for the signal from the software application containing playback. Match your recording software application's mixer output and the Software Return menu selection. In most cases, the recording software mixer output and Maestro's Software Return will be set to 1-2.
> > 9. Mixer Master - This is the level control and meter for the mixer's output.

#